NOTES:
1
27

11
20	Date Code located on gearcase near output spindle.

Torque to 9-11 Nm (80-97 in. lbs.).
Torque to 1.2-1.6 Nm (10.6-14.2 in. lbs.).	
19	Torque to 0.45-0.65 Nm (4-5.8 in. lbs.).	
21, 28	Torque to 1.2-1.4 Nm (10.6-12.4 in. lbs.).	
		
22	Torque to 0.9-1.1 Nm (8-9.7 in. lbs.).	

6,836

Continued-
6, 836 Cont’d

LUBRICATION:
7	Apply lubricant to O-ring for ease of assembly.	
9	Apply 15-17g (0.5 – 0.6 oz.) of grease to gear teeth.	

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.