NOTES:
1
8
11	Date Code located in Battery Foot area.
Torque to 0.9 ± 0.1 Nm (8.0 ± 1 in. lbs.).
Torque to 1.2 ± 0.1 Nm (10.5 ± 1 in. lbs.).	
13	Torque to 0.6 ± 0.1 Nm (5.0 ± 1 in. lbs.).	
23	Alternately tighten screws until screw torque is 7.9 ± 1.7 Nm (70 ± 15 in. lbs.).	

LUBRICATION:
21, 23	Apply 3.5g (0.125 oz.) of grease to back of head before assembly.	

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.