NOTES:
		  1	Place 0.017 Kg (0.5 ounces) grease in gear case cavity.
	    3, 5, 12	Torque screws 33-37 in-lbs.
		  5	Torque support plate screws 44-48 in-lbs.
	        8, 19	Torque screws 9-12 in-lbs.
		  9	Torque fan baffle screws 20-24 in-lbs.
15, 24, 28	Apply grease liberally to surfaces, pin, and bearing.
	            33	Torque screws 18-22 in-lbs.
	            40	Torque screws 12-16 in-lbs.
	            41	Torque screws 5-9 in-lbs.
	            48	Torque screws 25-29 in-lbs.

CAUTION:
Static electricity can damage electronic components. Repair only at a static-free station. Refer to SDB 5955. 
IMPORTANT:
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.