NOTES:
    1					The fence should be adjusted parallel within 0.13mm (.005”) to the right miter slot.
  1	The fence must be parallel to gage blade within 0.3mm with any gap occurring at the
back of the blade.  
    1 					Spacing between the right side fence rail pins can be checked and adjusted using the 
							holes in the blade wrenches. (4" for DWE7490X, 8" for DWE7491RS and DWE7499GD) 
12		   		Rip scale Indicator to be adjusted to match the zero mark on the scale. 
103,104 		Blade height rail adjustment:

110	   The bevel mechanism must be adjusted so that the supplied or “dummy” blade is parallel to the right
   miter slot within 0.2 mm maximum over a 200 mm length along the blade at 90° and within 0.4mm at
   45°.
134			 The bevel pointer shall be positioned so that the center mark points at 0 (0.25).  
180			 The bevel stops should be adjusted so that the supplied or “dummy” blade registers within 0.2 at 90 
					and 0.2 at 45.  
253			 The throat plate shall be adjusted:
Flush to 0.5 mm below with the table top at the front of the throat plate.
Flush to 0.7 mm above the table top at the rear of the throat plate. 

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.